

**DRAFT RESULTS – Undergoing Final Review**

**Draft Summary Port of Stockton 2018 Emissions Inventory**



**OGV Emissions by Mode**



Final results pending review by the Technical Working Group.

**1.1 Geographical Domain**

The geographical domain for each of the source categories is defined below.

* Ocean going vessels and harbor craft: the over-water geographic domain is within the SJVAPCD boundary which is the San Joaquin river from the confluence of the San Joaquin and Mokelumne rivers to the Port.
* Cargo handling equipment: the geographic domain is within the Port boundary.
* Locomotives: the geographic domain is within the Port boundary and from the Port boundary to the two class one switching yards (approximately 5 miles from the Port).
* On-road vehicles, heavy-duty vehicles: the geographic domain is from the Port to the entrance or exit of the Interstate 5 or State Route 4 freeways.
* On-road vehicles, Port owned on-road vehicles: actual miles traveled which includes mostly on-Port operation.